{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["F.1.1 分部分项工程和单价措施项目清单与计价表(表-08~"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"F.1.1 分部分项工程和单价措施项目清单与计价表(表-08~","index":0,"n_rows":35,"n_cols":11,"rows_kept":35,"merged":[[0,0,0,10],[1,0,1,1],[1,2,1,6],[1,7,1,8],[1,9,1,10],[2,0,4,0],[2,1,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,7],[2,8,2,10],[3,8,4,8],[3,9,4,9],[5,1,5,2],[5,6,5,7],[6,1,6,2],[6,6,6,7],[7,1,7,2],[7,6,7,7],[8,1,8,2],[8,6,8,7],[9,1,9,2],[9,6,9,7],[10,1,10,2],[10,6,10,7],[11,1,11,2],[11,6,11,7],[12,1,12,2],[12,6,12,7],[13,1,13,2],[13,6,13,7],[14,1,14,2],[14,6,14,7],[15,1,15,2],[15,6,15,7],[16,1,16,2],[16,6,16,7],[17,1,17,2],[17,6,17,7],[18,1,18,2],[18,6,18,7],[19,1,19,2],[19,6,19,7],[20,1,20,2],[20,6,20,7],[21,1,21,2],[21,6,21,7],[22,1,22,2],[22,6,22,7],[23,1,23,2],[23,6,23,7],[24,1,24,2],[24,6,24,7],[25,1,25,2],[25,6,25,7],[26,1,26,2],[26,6,26,7],[27,1,27,2],[27,6,27,7],[28,1,28,2],[28,6,28,7],[29,1,29,2],[29,6,29,7],[30,1,30,2],[30,6,30,7],[31,1,31,2],[31,6,31,7],[32,1,32,2],[32,6,32,7],[33,1,33,2],[33,6,33,7],[34,0,34,8]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表","","","","","","","","","",""]
["工程名称：","","动力2#地磅工程\\动力2#地磅工程【动力2#地磅工程】","","","","","标段：","","",""]
["序号","项目编码","","项目名称","项目特征","计量\r\n单位","工程\r\n量","","金额（元）","",""]
["","","","","","","","","综合单价","合价","其   中"]
["","","","","","","","","","","暂估价"]
["1","010103002069","","余方弃置（旧路沿石、人行道面层基层拆除）","1.废弃料品种 :土石方综合考虑（含清除表土、路沿石、人行道面层及基层）\r\n2.弃土运距：运距、弃土发生的城市道路清洁、卫生、环保、弃土场等一切费用均由投标人自行考虑\r\n3.弃土场地费：由投标人自行考虑\r\n4.其他：满足设计及现行技术、质量验收规范要求\r\n","m³ ","16.42","",null,null,""]
["2","040202011103","","100mm厚级配碎石层（新建道路）","1.垫层材料种类、厚度:100mm厚级配碎石\r\n2.具体要求:详设计施工图\r\n3.做法：满足设计及现行技术、质量验收规范要求","㎡","541.63","",null,null,""]
["3","040202011106","","400mm厚级配砂石层（新建引道）","1.垫层材料种类、厚度:400mm厚级配砂石\r\n2.具体要求:详设计施工图\r\n3.做法：满足设计及现行技术、质量验收规范要求\r\n","㎡","72","",null,null,""]
["4","040202012062","","300mm厚片石（新建道路）","1.石料规格及厚度:300mm厚片石层\r\n2.具体要求:详设计施工图\r\n3.做法：满足设计及现行技术、质量验收规范要求\r\n","㎡","541.63","",null,null,""]
["5","040203007059","","300mm厚C30混凝土路面（新建道路）","1.混凝土强度等级 ：商品砼C30\r\n2.厚度 ：300mm\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n","㎡","541.63","",null,null,""]
["6","040203007107","","250mm厚引道C30砼面层","1.混凝土强度等级 ：商品砼C30\r\n2.厚度 ：250mm\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n","㎡","72","",null,null,""]
["7","040204004066","","C25混凝土路缘石（新制安）","1.材料：C25砼\r\n2.尺寸：495×450×150mm\r\n3.形状：一字型、弧形\r\n4.粘接层：满足设计和规范要求，综合单价已包含粘接层\r\n5.含倒角、成品保护等\r\n6.具体要求:详设计施工图\r\n7.做法：满足设计及现行技术、质量验收规范要\r\n\r\n","m","141.2","",null,null,""]
["8","010501001081","","路缘石C20垫层","1.混凝土种类 ：商品砼\r\n2.混凝土强度等级：C20\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n","m³ ","4.22","",null,null,""]
["9","010501004104","","地磅C30基础砼","1.混凝土种类 ：商品砼\r\n2.混凝土强度等级：C30\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求","m³ ","38.34","",null,null,""]
["10","010503001117","","地磅C30基础梁","1.混凝土种类 ：商品砼\r\n2.混凝土强度等级：C30\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求","m³ ","3.36","",null,null,""]
["11","010501001074","","C20基础垫层砼","1.混凝土种类 ：商品砼\r\n2.混凝土强度等级：C20\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n","m³ ","7.27","",null,null,""]
["12","010516002093","","预埋铁件","1.钢材种类：预埋铁件\r\n2.做法：满足设计及现行技术、质量验收规范要求","t","0.082","",null,null,""]
["13","010516001102","","预埋螺栓","1.螺栓种类：高强镙栓M16（不含螺栓材料费）\r\n2.规格：综合\r\n3.做法：满足设计及现行技术、质量验收规范要求","套","32","",null,null,""]
["14","010515001055","","现浇构件钢筋 HRB400 ≤φ10 制作安装","1.钢筋种类、规格：现浇构件钢筋（HRB400 Φ10以内），钢筋牌号带“E”和不带“E”由投标人综合考虑在报价中\r\n2.钢筋除锈费用包括在综合单价内\r\n3.构件直形与弧形综合考虑\r\n4.投标人综合考虑埋设的方式,无论采用预留、植筋或其他方式施工,其所有费用均包括在所报综合单价中不再另行计取\r\n5.其他：满足设计及施工验收规范","t","0.996","",null,null,""]
["15","010515001071","","现浇构件钢筋 HRB400 φ12-16 制作安装","1.钢筋种类、规格：现浇构件钢筋（HRB400 Φ12-16以内），钢筋牌号带“E”和不带“E”由投标人综合考虑在报价中\r\n2.钢筋除锈费用包括在综合单价内\r\n3.构件直形与弧形综合考虑\r\n4.投标人综合考虑埋设的方式,无论采用预留、植筋或其他方式施工,其所有费用均包括在所报综合单价中不再另行计取\r\n5.其他：满足设计及施工验收规范","t","3.247","",null,null,""]
["16","010515001072","","现浇构件钢筋 HRB400 φ16以上制作安装","1.钢筋种类、规格：现浇构件钢筋（HRB400 Φ16以上），钢筋牌号带“E”和不带“E”由投标人综合考虑在报价中\r\n2.钢筋除锈费用包括在综合单价内\r\n3.构件直形与弧形综合考虑\r\n4.投标人综合考虑埋设的方式,无论采用预留、植筋或其他方式施工,其所有费用均包括在所报综合单价中不再另行计取\r\n5.其他：满足设计及施工验收规范","t","0.195","",null,null,""]
["17","041001005113","","拆除原有路沿石","1.名称： 路沿石拆除\r\n2.拆除构件的厚度或规格尺寸： 综合考虑\r\n3.构件的附着物及基层种类：土、砼等\r\n4.土、石渣场内运输方式及运距：投标人踏勘现场后自行确定，需结合实际并符合当地行政主管部门要求;","m","30.68","",null,null,""]
["18","041001002114","","拆除人行道面层及基层","1.名称：人行道面层及基层拆除\r\n2.拆除构件的厚度或规格尺寸： 综合考虑\r\n3.构件的附着物及基层种类：土、砼等\r\n4.土、石渣场内运输方式及运距：投标人踏勘现场后自行确定，需结合实际并符合当地行政主管部门要求;","㎡","61.36","",null,null,""]
["19","011601001109","","开窗洞砖砌体拆除","1.砌体名称： 砖墙\r\n2.砌体材质 ：实心页岩砖\r\n3.拆除高度：综合考虑\r\n4.拆除砌体的截面尺寸： 1.2m*1.2m\r\n5.砌体表面的附着物种类：综合考虑\r\n6.土、石渣场内运输方式及运距：投标人踏勘现场后自行确定，需结合实际并符合当地行政主管部门要求;","m³ ","0.35","",null,null,""]
["20","010807007112","","88系列塑钢窗推拉C1212","1.窗代号:C1212\r\n2.框外围展开面积:详设计\r\n3.框、扇材质 :88系列塑钢，窗型材满足泸州市节能备案要求企业品牌材料\r\n4.玻璃品种、厚度：5mm厚普通玻璃\r\n5.其它：未尽事宜满足设计及现行技术、质量验收规范要求","㎡","1.44","",null,null,""]
["21","030409002115","","热镀锌扁钢 40*4","1.名称：接地母线 -40*4热镀锌扁钢（地磅基础范围）\r\n2.材质：热镀锌扁钢\r\n3.规格：-40*4\r\n4.其他详见设计施工图、未尽事宜满足设计及现行技术、质量验收规范要求","m","42.68","",null,null,""]
["22","011701006","","满堂脚手架","1．搭设方式 \r\n2. 搭设高度 \r\n3．脚手架材质","㎡","64.98","",null,null,""]
["23","011702001","","地磅基础垫层模板","1.构件部位：垫层模板\r\n2.支模高度:综合\r\n3.模板类型:木模、组合钢模板、竹胶合板、复合模板综合\r\n4.支架材料:钢管、竹、木支架综合\r\n5.本项目投标人应根据设计图纸,投标施工组织设计,现场实际情况和企业自身情况综合报价,不论采用何种支模方式均执行该综合单价\r\n6.其他:满足设计及施工验收规范","㎡","4.59","",null,null,""]
["24","011702001","","地磅基础模板","基础类型","㎡","21.3","",null,null,""]
["25","041102002","","路缘石垫层模板","1.构件部位：路缘石基础模板\r\n2.支模高度:综合\r\n3.模板类型:木模、组合钢模板、竹胶合板、复合模板综合\r\n4.支架材料:钢管、竹、木支架综合\r\n5.本项目投标人应根据设计图纸,投标施工组织设计,现场实际情况和企业自身情况综合报价,不论采用何种支模方式均执行该综合单价\r\n6.其他:满足设计及施工验收规范","㎡","14.25","",null,null,""]
["26","自编清单","","新建道路砼面层模板\r\n"," ","㎡","541.63","",null,null,""]
["27","自编清单","","新建引道砼面层模板"," ","㎡","72","",null,null,""]
["28","011702005","","基础梁模板","梁截面形状","㎡","12.88","",null,null,""]
["29","011705001001","","大型机械设备进出场及安拆","1.机械设备名称：投标人自行考虑，费用综合在报价中 \r\n2.机械设备规格型号：投标人自行考虑，费用综合在报价中\r\n3.其余做法：满足施工及进度要求","项","1","",null,null,""]
["合　　计","","","","","","","","",null,""]