{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["F.1.1 分部分项工程清单计价表(表-08)不带分部【采样~","F.1.2 单价措施项目清单计价表(表-08)不带分部【采样~","G.2 暂列金额明细表(表-12-1)【采样机棚土建】"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"F.1.1 分部分项工程清单计价表(表-08)不带分部【采样~","index":0,"n_rows":46,"n_cols":11,"rows_kept":46,"merged":[[0,0,0,10],[1,0,1,1],[1,2,1,6],[1,7,1,8],[1,9,1,10],[2,0,4,0],[2,1,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,7],[2,8,2,10],[3,8,4,8],[3,9,4,9],[5,1,5,2],[5,6,5,7],[6,1,6,2],[6,6,6,7],[7,1,7,2],[7,6,7,7],[8,1,8,2],[8,6,8,7],[9,1,9,2],[9,6,9,7],[10,1,10,2],[10,6,10,7],[11,1,11,2],[11,6,11,7],[12,1,12,2],[12,6,12,7],[13,1,13,2],[13,6,13,7],[14,1,14,2],[14,6,14,7],[15,1,15,2],[15,6,15,7],[16,1,16,2],[16,6,16,7],[17,1,17,2],[17,6,17,7],[18,1,18,2],[18,6,18,7],[19,1,19,2],[19,6,19,7],[20,1,20,2],[20,6,20,7],[21,1,21,2],[21,6,21,7],[22,1,22,2],[22,6,22,7],[23,1,23,2],[23,6,23,7],[24,1,24,2],[24,6,24,7],[25,1,25,2],[25,6,25,7],[26,1,26,2],[26,6,26,7],[27,1,27,2],[27,6,27,7],[28,1,28,2],[28,6,28,7],[29,1,29,2],[29,6,29,7],[30,1,30,2],[30,6,30,7],[31,1,31,2],[31,6,31,7],[32,1,32,2],[32,6,32,7],[33,1,33,2],[33,6,33,7],[34,1,34,2],[34,6,34,7],[35,1,35,2],[35,6,35,7],[36,1,36,2],[36,6,36,7],[37,1,37,2],[37,6,37,7],[38,1,38,2],[38,6,38,7],[39,1,39,2],[39,6,39,7],[40,1,40,2],[40,6,40,7],[41,1,41,2],[41,6,41,7],[42,1,42,2],[42,6,42,7],[43,1,43,2],[43,6,43,7],[44,1,44,2],[44,6,44,7],[45,0,45,8]],"flags":["formulas_cached_only"]}
["分部分项工程量清单与计价表","","","","","","","","","",""]
["工程名称：","","采样机棚工程\\采样机棚工程【采样机棚土建】","","","","","标段：","","",""]
["序号","项目编码","","项目名称","项目特征描述","计量\r\n单位","工程量","","金额（元）","",""]
["","","","","","","","","综合单价","合价","其   中"]
["","","","","","","","","","","暂估价"]
["1","010101002082","","挖一般土石方","1.类别： 各类土(含淤泥)和各类石质综合\r\n2.开挖深度：综合\r\n3.开挖方式、运输方式、土石方调配：投标人踏勘现场后自行考虑\r\n4.场内运距：投标人踏勘现场后自行确定\r\n5.其他：未尽事宜需满足设计及现行技术、质量验收规范要求","m3","292.78","","","",""]
["2","010101003067","","挖沟槽土石方","1.土石类别：各类土(含淤泥)和各类石质综合\r\n2.基础类型：按设计施工图\r\n3.开挖或开凿深度：按设计要求\r\n4.基底摊座要求：底检平\r\n5.开挖方式：由投标人自行确定\r\n6.土、石渣场内运输方式及运距：投标人踏勘现场后自行确定，需结合实际并符合当地行政主管部门要求;\r\n7.做法：满足设计及现行施工技术、质量验收规范要求","m3","332.79","","","",""]
["3","010103001068","","回填方","1.密实度要求：分层机械压实,每层回填厚度不大于300,检测合格后方可进行上一层回填，回填土压实系数不小于0.95\r\n2.填方材料品种：满足设计及规范要求\r\n3.填方粒径要求：满足设计及规范要求\r\n4.填方来源、运距：投标人综合考虑买土回填、原土回填等，结算时无论采用何种回填方式，综合单价不作调整，填方场内外运距由投标人自行考虑\r\n5.其它：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","m3","93.67","","","",""]
["4","010103002069","","余方弃置","1.废弃料品种 :土石方综合考虑（含清除表土）\r\n2.弃土运距：运距、弃土发生的城市道路清洁、卫生、环保、弃土场等一切费用均由投标人自行考虑\r\n3.弃土场地费：由投标人自行考虑\r\n4.其他：满足设计及现行技术、质量验收规范要求\r\n","m3","531.9","","","",""]
["5","040202011103","","100mm厚级配碎石层（道路、人行道）","1.垫层材料种类、厚度:100mm厚级配碎石\r\n2.具体要求:详设计施工图\r\n3.做法：满足设计及现行技术、质量验收规范要求","m2","432.97","","","",""]
["6","040202011104","","60mm厚级配碎石层（地坪）","1.垫层材料种类、厚度:60mm厚级配碎石\r\n2.具体要求:详设计施工图\r\n3.做法：满足设计及现行技术、质量验收规范要求","m2","145.75","","","",""]
["7","040202012062","","300mm厚片石（道路）","1.石料规格及厚度:300mm厚片石层\r\n2.具体要求:详设计施工图\r\n3.做法：满足设计及现行技术、质量验收规范要求\r\n","m2","336.44","","","",""]
["8","040203007059","","300mm厚C30混凝土路面（道路）","1.混凝土强度等级 ：商品砼C30\r\n2.厚度 ：300mm\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n","m2","336.44","","","",""]
["9","040204003065","","100mm厚C25混凝土人行道及进口坡路面","1.混凝土强度等级 ：商品砼C25\r\n2.厚度 ：100mm\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n\r\n\r\n","m2","96.53","","","",""]
["10","010507002096","","100mm厚C25混凝土室外地坪","1.混凝土强度等级 ：商品砼C25\r\n2.厚度 ：100mm\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n","m2","145.75","","","",""]
["11","040204004066","","C25混凝土路缘石","1.材料：C25砼\r\n2.尺寸：495×450×150mm\r\n3.形状：一字型、弧形\r\n4.粘接层：满足设计和规范要求，综合单价已包含粘接层\r\n5.含倒角、成品保护等\r\n6.具体要求:详设计施工图\r\n7.做法：满足设计及现行技术、质量验收规范要\r\n\r\n","m","152.49","","","",""]
["12","010501001081","","路缘石C20基础","1.混凝土种类 ：商品砼\r\n2.混凝土强度等级：C20\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n","m3","8.58","","","",""]
["13","010501006036","","C30设备基础","1.混凝土种类 ：商品砼\r\n2.混凝土强度等级：C30\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n","m3","30.31","","","",""]
["14","010101004101","","挖基坑土石方（采样装置基础部分）","1.土石类别：各类土(含淤泥)和各类石质综合\r\n2.基础类型：按设计施工图\r\n3.开挖或开凿深度：按设计要求\r\n4.基底摊座要求：底检平\r\n5.开挖方式：由投标人自行确定\r\n6.土、石渣场内运输方式及运距：投标人踏勘现场后自行确定，需结合实际并符合当地行政主管部门要求;\r\n7.做法：满足设计及现行施工技术、质量验收规范要求","m3","195.84","","","",""]
["15","010103001068","","回填方（采样装置部分基础部分）","1.密实度要求：分层机械压实,每层回填厚度不大于300,检测合格后方可进行上一层回填，回填土压实系数不小于0.95\r\n2.填方材料品种：满足设计及规范要求\r\n3.填方粒径要求：满足设计及规范要求\r\n4.填方来源、运距：投标人综合考虑买土回填、原土回填等，结算时无论采用何种回填方式，综合单价不作调整，填方场内外运距由投标人自行考虑\r\n5.其它：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","m3","153.09","","","",""]
["16","010103002069","","余方弃置（采样装置部分基础部分）","1.废弃料品种 :土石方综合考虑（含清除表土）\r\n2.弃土运距：运距、弃土发生的城市道路清洁、卫生、环保、弃土场等一切费用均由投标人自行考虑\r\n3.弃土场地费：由投标人自行考虑\r\n4.其他：满足设计及现行技术、质量验收规范要求\r\n","m3","196.5","","","",""]
["17","010501001074","","C15基础垫层","1.混凝土种类 ：商品砼\r\n2.混凝土强度等级：C15\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n","m3","8.16","","","",""]
["18","010516002093","","预埋铁件","1.钢材种类：预埋铁件\r\n2.做法：满足设计及现行技术、质量验收规范要求","t","0.365","","","",""]
["19","010516001092","","预埋螺栓\r\n\r\n螺栓"," ","t","0","","","",""]
["20","010516001102","","地脚螺栓","1.螺栓种类：高强镙栓（不含螺栓材料费）\r\n2.规格：综合\r\n3.做法：满足设计及现行技术、质量验收规范要求","套","48","","","",""]
["21","010501003045","","C35独立基础","1.混凝土种类 ：商品砼\r\n2.混凝土强度等级：C35\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n","m3","28.96","","","",""]
["22","010502001099","","C35矩形柱 ","1.混凝土种类 ：商品砼\r\n2.混凝土强度等级：C35\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求\r\n","m3","5.37","","","",""]
["23","010507007086","","C20素混凝土包裹柱脚","1.混凝土种类 ：满足设计和规范要求\r\n2.混凝土强度等级：C20素混凝土包裹柱脚\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求","m3","1.04","","","",""]
["24","010507007100","","C40无收缩细石砼灌缝","1.混凝土种类 ：满足设计和规范要求\r\n2.混凝土强度等级：C40无收缩细石砼灌缝\r\n3.砼现场浇筑方式及机械种类：投标人自行考虑，费用包含在投标报价中\r\n4.具体要求:详设计施工图\r\n5.做法：满足设计及现行技术、质量验收规范要求","m3","0.27","","","",""]
["25","010515001055","","现浇构件钢筋 HRB400 ≤φ10 制作安装","1.钢筋种类、规格：现浇构件钢筋（HRB400 Φ10以内），钢筋牌号带“E”和不带“E”由投标人综合考虑在报价中\r\n2.钢筋除锈费用包括在综合单价内\r\n3.构件直形与弧形综合考虑\r\n4.投标人综合考虑埋设的方式,无论采用预留、植筋或其他方式施工,其所有费用均包括在所报综合单价中不再另行计取\r\n5.其他：满足设计及施工验收规范","t","0.033","","","",""]
["26","010515001071","","现浇构件钢筋 HRB400 φ12-16 制作安装","1.钢筋种类、规格：现浇构件钢筋（HRB400 Φ12-16以内），钢筋牌号带“E”和不带“E”由投标人综合考虑在报价中\r\n2.钢筋除锈费用包括在综合单价内\r\n3.构件直形与弧形综合考虑\r\n4.投标人综合考虑埋设的方式,无论采用预留、植筋或其他方式施工,其所有费用均包括在所报综合单价中不再另行计取\r\n5.其他：满足设计及施工验收规范","t","1.152","","","",""]
["27","010515001072","","现浇构件钢筋 HRB400 φ16以上制作安装","1.钢筋种类、规格：现浇构件钢筋（HRB400 Φ16以上），钢筋牌号带“E”和不带“E”由投标人综合考虑在报价中\r\n2.钢筋除锈费用包括在综合单价内\r\n3.构件直形与弧形综合考虑\r\n4.投标人综合考虑埋设的方式,无论采用预留、植筋或其他方式施工,其所有费用均包括在所报综合单价中不再另行计取\r\n5.其他：满足设计及施工验收规范","t","0.518","","","",""]
["28","010604001075","","钢梁（主梁）","1.梁类型：H型钢 （不含成品H型钢梁、螺栓材料费）\r\n2.钢材品种、规格：详设计图  \r\n3.单根质量：≤10t\r\n4.安装高度 ：详设计图\r\n5.防火要求,耐火极限满足设计要求（另列）\r\n6.探伤要求：二级 \r\n7.其他：满足设计及施工验收规范\r\n","t","4.544","","","",""]
["29","010604002076","","钢吊车梁","1.梁类型：钢吊车梁（不含成品钢吊车梁、螺栓材料费）\r\n2.钢材品种、规格：详设计图  \r\n3.单根质量：综合 \r\n4.安装高度 ：详设计图\r\n5.防火要求,耐火极限满足设计要求（另列）\r\n6.探伤要求：二级 \r\n7.其他：满足设计及施工验收规范\r\n","t","3.683","","","",""]
["30","010604001077","","钢梁（主梁除外）","1.梁类型：综合， 主梁除外（不含钢梁、螺栓材料费）\r\n2.钢材品种、规格：详设计图 \r\n3.单根质量：综合\r\n4.安装高度 ：详设计图\r\n5.防火要求,耐火极限满足设计要求（另列）\r\n6.探伤要求：二级 \r\n7.其他：满足设计及施工验收规范\r\n","t","0.859","","","",""]
["31","010603001085","","实腹钢柱","1.柱类型：H型钢 （不含成品钢板焊接H形钢柱、螺栓材料费）\r\n2.钢材品种、规格：详设计图  \r\n3.单根质量：≤10t\r\n4.安装高度 ：详设计图\r\n5.防火要求,耐火极限满足设计要求（另列）\r\n6.探伤要求：二级 \r\n7.其他：满足设计及施工验收规范\r\n","t","11.626","","","",""]
["32","010602003084","","车挡板\r\n","1.构件类型：车挡板 （不含车挡板钢材、螺栓材料费）\r\n2.钢材品种、规格：详设计图  \r\n3.单根质量：综合\r\n4.安装高度 ：详设计图\r\n5.防火要求,耐火极限满足设计要求（另列）\r\n6.探伤要求：二级 \r\n7.其他：满足设计及施工验收规范\r\n","t","0.449","","","",""]
["33","010606001087","","钢支撑、钢拉条","1.构件类型：钢支撑、钢拉条（不含成品型钢钢支撑、螺栓材料费）\r\n2.钢材品种、规格：详设计图  \r\n3.单根质量：综合\r\n4.安装高度 ：详设计图\r\n5.防火要求,耐火极限满足设计要求（另列）\r\n6.探伤要求：二级 \r\n7.其他：满足设计及施工验收规范\r\n","t","4.765","","","",""]
["34","010606002088","","钢檩条","1.构件类型：钢檩条（不含成品型钢钢檩条、螺栓材料费）\r\n2.钢材品种、规格：详设计图  \r\n3.单根质量：综合\r\n4.安装高度 ：详设计图\r\n5.防火要求,耐火极限满足设计要求（另列）\r\n6.探伤要求：二级 \r\n7.其他：满足设计及施工验收规范\r\n","t","1.901","","","",""]
["35","010606009089","","钢护栏","1.构件类型：钢护栏（不含成品钢管栏杆材料费）\r\n2.钢材品种、规格：详设计图  \r\n3.单根质量：综合\r\n4.安装高度 ：详设计图\r\n5.防火要求,耐火极限满足设计要求（另列）\r\n6.探伤要求：二级 \r\n7.其他：满足设计及施工验收规范\r\n","t","1.514","","","",""]
["36","010606012090","","钢支架","1.构件类型：钢支架（不含成品钢支架、螺栓材料费）\r\n2.钢材品种、规格：详设计图  \r\n3.单根质量：综合\r\n4.安装高度 ：详设计图\r\n5.防火要求,耐火极限满足设计要求（另列）\r\n6.探伤要求：二级 \r\n7.其他：满足设计及施工验收规范\r\n","t","0.043","","","",""]
["37","010606008094","","钢梯","1.构件类型：钢梯（不含成品踏步式扶梯、螺栓材料费）\r\n2.钢材品种、规格：详设计图  \r\n3.单根质量：综合\r\n4.安装高度 ：详设计图\r\n5.防火要求,耐火极限满足设计要求（另列）\r\n6.探伤要求：二级 \r\n7.其他：满足设计及施工验收规范\r\n","t","0.779","","","",""]
["38","010606006095","","钢平台","1.构件类型：钢平台（不含成品钢操作台、螺栓材料费）\r\n2.钢材品种、规格：详设计图  \r\n3.单根质量：综合\r\n4.安装高度 ：详设计图\r\n5.防火要求,耐火极限满足设计要求（另列）\r\n6.探伤要求：二级 \r\n7.其他：满足设计及施工验收规范\r\n","t","1.235","","","",""]
["39","010605002097","","墙板","1.钢材品种、规格 ：YX24-210-840型压型钢板（不含墙面压型钢板、螺栓、铆钉、垫圈材料费）\r\n2.钢板厚度、复合板厚度：0.5mm厚度\r\n3.其他：防水等级II级,压型钢板自防水\r\n4.做法满足设计及施工验收规范\r\n","m2","237.77","","","",""]
["40","010605001098","","屋面板","1.屋面板钢材品种、规格及厚度：详设计图\r\n3.其他：不含屋面钢板、固定架、螺栓、堵头、挡雨板、屋脊板、包角板材料费\r\n4.做法满足设计及施工验收规范\r\n","m2","209.33","","","",""]
["合　　计","","","","","","","","","",""]

{"sheet":"F.1.2 单价措施项目清单计价表(表-08)不带分部【采样~","index":1,"n_rows":14,"n_cols":11,"rows_kept":14,"merged":[[0,0,0,10],[1,0,1,1],[1,2,1,6],[1,7,1,8],[1,9,1,10],[2,0,4,0],[2,1,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,7],[2,8,2,10],[3,8,4,8],[3,9,4,9],[5,1,5,2],[5,6,5,7],[6,1,6,2],[6,6,6,7],[7,1,7,2],[7,6,7,7],[8,1,8,2],[8,6,8,7],[9,1,9,2],[9,6,9,7],[10,1,10,2],[10,6,10,7],[11,1,11,2],[11,6,11,7],[12,1,12,2],[12,6,12,7],[13,0,13,8]],"flags":["formulas_cached_only"]}
["单价措施项目清单与计价表","","","","","","","","","",""]
["工程名称：","","采样机棚工程\\采样机棚工程【采样机棚土建】","","","","","标段：","","",""]
["序 号","项目编码","","项目名称","项目特征描述","计量\r\n单位","工程量","","金额（元）","",""]
["","","","","","","","","综合单价","合价","其中"]
["","","","","","","","","","","暂估价"]
["1","011701001","","综合脚手架","1.建筑结构形式：钢结构 \r\n2.檐口高度：详设计\r\n3.现场施工若采用其他措施代替综合脚手架功能，结算时综合单价不做调整","m2","178.5","","","",""]
["2","011701002001","","外脚手架","1.双排脚手架\r\n2.搭设高度约9米","m2","0","","","",""]
["3","011702001","","基础垫层","1.构件部位：垫层模板\r\n2.支模高度:综合\r\n3.模板类型:木模、组合钢模板、竹胶合板、复合模板综合\r\n4.支架材料:钢管、竹、木支架综合\r\n5.本项目投标人应根据设计图纸,投标施工组织设计,现场实际情况和企业自身情况综合报价,不论采用何种支模方式均执行该综合单价\r\n6.其他:满足设计及施工验收规范","m2","10.24","","","",""]
["4","011702001","","独立基础","1.构件部位：独立基础模板\r\n2.支模高度:综合\r\n3.模板类型:木模、组合钢模板、竹胶合板、复合模板综合\r\n4.支架材料:钢管、竹、木支架综合\r\n5.本项目投标人应根据设计图纸,投标施工组织设计,现场实际情况和企业自身情况综合报价,不论采用何种支模方式均执行该综合单价\r\n6.其他:满足设计及施工验收规范","m2","28.8","","","",""]
["5","011702002","","矩形柱","1.构件部位：矩形柱模板\r\n2.支模高度:综合\r\n3.模板类型:木模、组合钢模板、竹胶合板、复合模板综合\r\n4.支架材料:钢管、竹、木支架综合\r\n5.本项目投标人应根据设计图纸,投标施工组织设计,现场实际情况和企业自身情况综合报价,不论采用何种支模方式均执行该综合单价\r\n6.其他:满足设计及施工验收规范","m2","27.04","","","",""]
["6","011702025","","其它现浇构件（二次浇筑C20、C40）","1.构件部位：其它现浇构件模板\r\n2.支模高度:综合\r\n3.模板类型:木模、组合钢模板、竹胶合板、复合模板综合\r\n4.支架材料:钢管、竹、木支架综合\r\n5.本项目投标人应根据设计图纸,投标施工组织设计,现场实际情况和企业自身情况综合报价,不论采用何种支模方式均执行该综合单价\r\n6.其他:满足设计及施工验收规范","m2","6.6","","","",""]
["7","041102002","","路缘石基础模板","1.构件部位：路缘石基础模板\r\n2.支模高度:综合\r\n3.模板类型:木模、组合钢模板、竹胶合板、复合模板综合\r\n4.支架材料:钢管、竹、木支架综合\r\n5.本项目投标人应根据设计图纸,投标施工组织设计,现场实际情况和企业自身情况综合报价,不论采用何种支模方式均执行该综合单价\r\n6.其他:满足设计及施工验收规范","m2","83.87","","","",""]
["8","011705001001","","大型机械设备进出场及安拆","1.机械设备名称：投标人自行考虑，费用综合在报价中 \r\n2.机械设备规格型号：投标人自行考虑，费用综合在报价中\r\n3.其余做法：满足施工及进度要求","项","1","","","",""]
["合　　计","","","","","","","","","",""]

{"sheet":"G.2 暂列金额明细表(表-12-1)【采样机棚土建】","index":2,"n_rows":5,"n_cols":5,"rows_kept":5,"merged":[[0,0,0,4],[1,2,1,3],[4,0,4,2]],"flags":["formulas_cached_only"]}
["暂列金额明细表","","","",""]
["工程名称：","采样机棚工程\\采样机棚工程【采样机棚土建】","标段：","",""]
["序号","项目名称","计量单位","暂定金额(元)","备注"]
["1","暂列金额","项","31016.74"," "]
["合　　计","","","31016.74","-"]